Cells and batteries which, in accordance with special provision 376, are identified as damaged or defective and liable to rapidly disassemble, dangerously react, produce a flame or a dangerous evolution of heat or a dangerous emission of toxic, corrosive or flammable gases or vapours under normal conditions of carriage, shall be assigned to transport category 0. In the transport document, the words "CARRIAGE IN ACCORDANCE WITH SPECIAL PROVISION 376" shall be supplemented by the words "TRANSPORT CATEGORY 0".