Formulations which in laboratory testing neither detonate in the cavitated state nor deflagrate, which show no effect when heated under confinement and which exhibit no explosive power may be transported under this entry. The formulation must also be thermally stable (i.e. the SADT is 60°C or higher for a 50 kg package).Formulations not meeting these criteria shall be transported under the provisions of Division 5.2; see 2.5.3.2.4.