This substance is listed in tank instruction T23 in 4.2.5.2.6 of the UN Model Regulations.

The carriage of peroxyacetic acid, Type F in packagings is also possible under UN No. 3109 under BAM Nos. 6716 and 9023.