See remarks 13) and 14) on the table in 2.5.3.2.4:

13) "CORROSIVE" subsidiary hazard label required (Model No 8, see 5.2.2.2.2).

14) Peroxyacetic acid formulations which fulfil the criteria of 2.5.3.3.2 (d).