Für die Zusatzgefahr siehe 2.0.5.6:
Subsidiary hazards shall be representative of the primary hazard posed by the other dangerous goods contained within the article or they shall be the subsidiary hazard(s) identified in column 4 of the Dangerous Goods List when only one dangerous good is present in the article. If the article contains more than one dangerous good and these could react dangerously with one another during transport, each of the dangerous goods shall be enclosed separately (see 4.1.1.6).