Petroleum crude oil containing hydrogen sulphide in sufficient concentration that vapours evolved from the crude oil can present an inhalation hazard shall be consigned under the entry UN3494 PETROLEUM CRUDE OIL, FLAMMABLE, TOXIC.