An oxygen generator, chemical, containing oxidizing substances shall meet the following conditions:

(a)	The generator when containing an explosive actuating device shall only be transported under this entry when excluded from Class 1 in accordance with paragraph 2.1.1.1 (b) of these Regulations;

(b)	The generator, without its packaging, shall be capable of withstanding a 1.8 m drop test onto a rigid, non-resilient, flat and horizontal surface, in the position most likely to cause damage, without loss of its contents and without actuation; and

(c)	When a generator is equipped with an actuating device, it shall have at least two positive means of preventing unintentional actuation.