Phthalic anhydride in the solid state and tetrahydrophthalic anhydrides, with not more than 0.05% maleic anhydride, are not subject to these Regulations.
Phthalic anhydride molten at a temperature above its flash point, with not more than 0.05% maleic anhydrides, shall be classified under UN 3256.