Carriage of this substance is permitted in tanks only.
Please note special provision 252: The solution must contain at least 7% water and shall contain not more than 0.2% combustible material. The chloride ion level shall not exceeds 0.02%.