See remarks 13) and 16) on the table in 2.5.3.2.4:

13) "CORROSIVE" subsidiary hazard label required (Model No. 8, see 5.2.2.2.2.

16)  Peroxyacetic acid formulations which fulfil the criteria of 2.5.3.3.2 (f).