This substance is not permitted for transport in portable tanks, or intermediate bulk containers with a capacity exceeding 450 litres, due to the potential initiation of an explosion when transported in large volumes.