Substances of packing group II or III with one or more subsidiary hazard(s) other than 6.1 and 8 may not be transported or handed over for transportation in portable tanks in the molten state according to 4.2.1.19 of the UN Model Regulations because the assigned tank instruction in column 10 of the Dangerous Goods List does not refer to transportation of the substance above its melting point.

Carriage of this substance in the molten state is therefore prohibited.