	Surveillance protocol according to BAM-GGR 001
Bags
	



	Surveillance protocol no.
	     

	to surveillance visit report no.
	     



	1 Review of the company’s self-monitoring by the surveillance assessor
(tests and test frequencies according to BAM-GGR 001)

	The self-monitoring documentation was checked at random:

	Design type/s/
approval certificate no/s.:
	     

	Production period/s:
	     

	Tests
	Testing frequency
	Result

	
	Minimum
	Actual
	(see footer)
	OK

	Materials, i.e. plastics granules, paper
	1/delivery
	     
	     
	|_|

	only in case of external supplier:
Finished and semi-finished goods, e.g. flat film
	1/delivery
	     
	     
	|_|

	Testing of individual layers
(type, grammage, sequence)
	1/(8 h) or
1/ lot
	     
	     
(only 1, 2, 3)
	|_|

	Dimensions
(e.g. functional dimensions, wall thickness)
	1/(4 h) or
1/ lot
	     
	     
(only 1, 2, 3)
	|_|

	Visual checks
(seams)
	1/(4 h) or
1/ lot
	     
	     
(only 1, 2, 3)
	|_|

	Gaskets/closures/valves
(correct assembly and function)
	1/(4 h) or
1/ lot
	     
	     
(only 1, 2, 3)
	|_|

	Marks
(correctness, readability, durability)
	1/(8 h) or
1/ lot
	     
	     
(only 1, 2, 3)
	|_|

	Drop testa
	(2/lot und 1/20.000) or
1/100b or
1/(24 months)b
	     
	     
(only 1, 2, 3)
	|_|

	Notes:
a = with a single sample the repeated drop testing according to ADR is carried out
b = special regulation for smallest batches: production of a design type < 100 pieces/year

	Comment:      

	2 Tests (according to ADR)
by the company in presence of the surveillance assessor

	|_| Tests (according to ADR) are carried out completely or in part by an external body
(please complete 2.1a in this case)

	2.1 Testing facilities and measuring equipment for internal tests (according to ADR)

	Were there any changes to the testing facilities since last surveillance visit?
	|_| yes
	|_| no

	Comment:      

	Review of the …
	(see footer)
	OK

	testing facilities (availability and suitability)
	     
(only 1, 2, 3)
	|_|

	measuring equipment (availability and suitability [type and calibration range])
	     
(only 1, 2, 3)
	|_|

	only for paper bags: air conditioning (availability)
	     
(only 1)
	|_|

	Comment:      

	2.1a External testing (according to ADR), if applicable

	Which external body (name, place) is carrying out tests (according to ADR) on behalf of the company?

	     

	Is this external body named in the recognized QAP?
	|_| no
	|_| yes

	Comment:      

	2.2 Drop test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Gross mass / kg
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Filling good
	     
	     
	     
(only 0, 1)
	|_|

	Drop height / m
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Drop orientation
	|_| flat on a wide face, a narrow face and an end
|_| flat on a wide face and an end
	     
(only 1, 2, 3)
	|_|

	Loss of filling good
	no
	     
	     
(only 3)
	|_|

	|_| class 1 goods
	→ no crack
	     
	     
(only 0, 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	3 Verification of design type conformity
by the surveillance assessor (for one design type)

	3.1 UN mark (and requirements as stated in the approval, if applicable)
	Result

	(alternatively, photographs can be submitted, marking height shall be stated)
	(see footer)
	OK

	UN mark
	see below photo 
	     
(only 1, 2, 3)
	|_|

	   font height / mm
	     
	     
(only 1)
	|_|

	Comment:      

	Photo of UN mark

	
Note: Photos must be trimmed to the relevant area before insertion, as this is not possible in the model template. Depending on the design type, additional photos of the stacking load pictogram, date clock, bottom mark, etc. can be inserted.

	3.2 Verification of the specification of this design type
(e.g. design (according to the technical drawing incl. drawing number and incl. revision date/status), material properties, closures (if applicable), dimensions incl. tolerances, tare mass)

	Characteristic checked
	Target
	Actual
	Result

	
	as per approval
	
	(see footer)
	OK

	Design
drawing/sample/type comparison
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	Additionally used documents:

	Approval certificate no.
incl. revision date/status
	     

	Design type test report no.
	     

	Comment:      

	Which documentation is provided by the company to the user of this design type, e.g. packaging or closing instruction?

	Comment:      
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