	Surveillance protocol according to BAM-GGR 001
Fibreboard boxes
	



	Surveillance protocol no.
	     

	to surveillance visit report no.
	     



	1 Review of the company’s self-monitoring by the surveillance assessor
(tests and test frequencies according to BAM-GGR 001)

	The self-monitoring documentation was checked at random:

	Design type/s/
approval certificate no/s.:
	     

	Production period/s:
	     

	Tests
	Testing frequency
	Result

	
	Minimum
	Actual
	(see footer)
	OK

	Materials, i.e. paper
	1/delivery
	     
	     
	|_|

	only in case of external supplier:
Finished and semi-finished goods, i.e. corrugated boarda
	1/delivery
	     
	     
	|_|

	Testing of individual layersb
(type, grammage, sequence)
	1/batchc or
1/lotd
	     
	     
(only 1, 2, 3)
	|_|

	Cobb1800 value
ISO 535, 1 individual test
≤ 155 g/m²
	1/batchc or
1/lotd
	     
	     
(only 1, 2, 3)
	|_|

	Puncture resistance
DIN 53142-1 or -2, 10 individual tests, 5/side
tolerance based on average value: -10 %
	1/batchc or
1/lotd
	     
	     
(only 1, 2, 3)
	|_|

	Bursting strength
ISO 2759, 10 individual tests, 5/side
tolerance based on average value: -10 %
	1/batchc or
1/lotd
	     
	     
(only 1, 2, 3)
	|_|

	Dimensions
(e.g. functional dimensions, wall thickness)
	1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Visual checks
(manufacturer seam, quality of the creasing)
	1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Mass of finished packaginge
	1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Marks
(correctness, readability, durability)
	1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Drop test …
|_| with PE bag filled with granulesf or
|_| other original inner packaging/s
	1/lot or
1/100g or
1/(24 months)g
	     
	     
(only 1, 2, 3)
	|_|

	|_| Stacking test (ADR) or
|_| Compression test (BCT)
DIN 55440-1, 5 individual tests
tolerance based on average value: -10 %
	1/lot or
1/100g or
1/(24 months)g
	     
	     
(only 1, 2, 3)
	|_|

	Notes:
a = bought-in corrugated board sheets (sheet material) shall be considered as semi-finished good
b = during/after processing an inspection for correct sequence of the basic material is sufficient; specification of the paper grade parameters only required, if not already considered during incoming goods control
c = when testing the still to be processed corrugated board batch (supplied batch)
d = when testing the ready-for-shipment packaging (production lot)
e = calculation of overall mass by summing up the mass of the individual parts allowed
f = incl. documentation of the length of the crack, if there is one; in % of the length of the packaging edge having that crack
g = special regulation for smallest batches: production of a design type < 100 pieces/year

	Comment:      

	2 Tests (according to ADR)
by the company in presence of the surveillance assessor

	|_| Tests (according to ADR) are carried out completely or in part by an external body
(please complete 2.1a in this case)

	2.1 Testing facilities and measuring equipment for internal tests (according to ADR)

	Were there any changes to the testing facilities since last surveillance visit?
	|_| yes
	|_| no

	Comment:      

	Review of the …
	(see footer)
	OK

	testing facilities (availability and suitability)
	     
(only 1, 2, 3)
	|_|

	measuring equipment (availability and suitability [type and calibration range])
	     
(only 1, 2, 3)
	|_|

	air conditioning (availability)
	     
(only 1)
	|_|

	standards regarding material testing (availability, currency)
	     
(only 1, 2)
	|_|

	Comment:      

	2.1a External testing (according to ADR), if applicable

	Which external body (name, place) is carrying out tests (according to ADR) on behalf of the company?

	     

	Is this external body named in the recognized QAP?
	|_| no
	|_| yes

	Comment:      

	2.2 Drop test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Gross mass / kg
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Drop height / m
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Drop orientation
	|_| flat on the bottom
|_| flat on the top
|_| flat one the long side
|_| flat on the short side
|_| on a corner
	     
(only 1, 2, 3)
	|_|

	Loss of filling good
	no
	     
	     
(only 3)
	|_|

	Filling good and crack length:
|_| with PE bag filled with granules
|_| other original inner packaging/s
|_| class 1 goods
	
→ ≤ 1/3 of LE
→ n.a.
→ no crack
	     
	     
(only 1, 2, 3)
	|_|

	note: LE = Length of the edge (of the packaging), having the crack

	Temperature of filling good / °C
	≤ -18
	     
	     
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	2.3 Stacking test/Compression test (BCT)

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	|_| Stacking load / kg
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Loss of filling good
	no
	     
	     
(only 3)
	|_|

	|_| Compression resistance / N
	≥ (      	- 10 %)
	     
	     
(only 1, 2, 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	3 Verification of design type conformity
by the surveillance assessor (for one design type)

	3.1 UN mark (and requirements as stated in the approval, if applicable)
	Result

	(alternatively, photographs can be submitted, marking height shall be stated)
	(see footer)
	OK

	UN mark
	see below photo 
	     
(only 1, 2, 3)
	|_|

	   font height / mm
	     
	     
(only 1)
	|_|

	Comment:      

	Photo of UN mark

	
Note: Photos must be trimmed to the relevant area before insertion, as this is not possible in the model template. Depending on the design type, additional photos of the stacking load pictogram, date clock, bottom mark, etc. can be inserted.

	3.2 Verification of the specification of this design type
(e.g. design (according to the technical drawing incl. drawing number and incl. revision date/status), material properties, adhesive tape, strapping band, dimensions incl. tolerances, tare mass)

	Characteristic checked
	Target
	Actual
	Result

	
	as per approval
	
	(see footer)
	OK

	Design
drawing/sample/type comparison
	     
	     
	     
(only 1, 2, 3)
	|_|

	Cobb1800 value
	≤ 155 g/m²
	     
	     
(only 3)
	|_|

	Bursting strength
	≥ (      	- 10 %)
	     
	     
(only 2)
	|_|

	Puncture resistance
	≥ (      	- 10 %)
	     
	     
(only 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	Additionally used documents:

	Approval certificate no.
incl. revision date/status
	     

	[bookmark: _Hlk496770095](Initial) Design type test report no.
	     

	if relevant:
Test protocol no.
	     

	if relevant:
Short test protocol no.
	     

	Comment:      

	Which documentation is provided by the company to the user of this design type, e.g. packaging or closing instruction?

	Description:      



	
[bookmark: _Hlk185497376][bookmark: _Hlk185498074]0 = not applicable, 1 = minor non-conformity 2 = serious non-conformity, 
[bookmark: _Hlk501695065]3 = safety-relevant non-conformity | recommendations can always be added in the comments field 	
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