	Surveillance protocol according to BAM-GGR 001
Flexible IBCs
	



	Surveillance protocol no.
	     

	to surveillance visit report no.
	     



	1 Review of the company’s self-monitoring by the surveillance assessor
(tests and test frequencies according to BAM-GGR 001)

	The self-monitoring documentation was checked at random:

	Design type/s/
approval certificate no/s.:
	     

	Production period/s:
	     

	Tests
	Testing frequency
	Result

	
	Minimum
	Actual
	(see footer)
	OK

	Materials, i.e. plastics raw material
	1/delivery
	     
	     
	|_|

	only in case of external supplier:
Finished and semi-finished goods, e.g. foils
	1/delivery
	     
	     
	|_|

	Dimensions
(e.g. functional dimensions, wall thickness)
	1/250 or
1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Visual checksa
(e.g. joints, seams, inner condition)
	each
	     
	     
(only 1, 2, 3)
	|_|

	Gaskets/closures/valves
(correct assembly and function)
	1/250 or
1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Marks
(correctness, readability, durability)
	1/1000 or
1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Drop testb
	1/1000 or
1/year
	     
	     
	|_|

	Top lift test
	1/1000 or
1/year
	     
	     
	|_|

	Topple test
	1/1000 or
1/year
	     
	     
	|_|

	Righting test
	1/1000 or
1/year
	     
	     
	|_|

	Notes:
a = inspection of the outer casing for non-conformities, especially such non-conformities, which can damage the inner receptacle, and of the fastening elements (welding seams, joints etc.)
b = tests, carried out in course of an additional design type test for a revision of the approval, can be included

	Comment:      

	2 Tests (according to ADR)
by the company in presence of the surveillance assessor

	|_| Tests (according to ADR) are carried out completely or in part by an external body
(please complete 2.1a in this case)

	2.1 Testing facilities and measuring equipment for internal tests (according to ADR)

	Were there any changes to the testing facilities since last surveillance visit?
	|_| yes
	|_| no

	Comment:      

	Review of the …
	(see footer)
	OK

	testing facilities (availability and suitability)
	     
(only 1, 2, 3)
	|_|

	measuring equipment (availability and suitability [type and calibration range])
	     
(only 1, 2, 3)
	|_|

	Comment:      

	2.1a External testing (according to ADR), if applicable

	Which external body (name, place) is carrying out tests (according to ADR) on behalf of the company?

	     

	Is this external body named in the recognized QAP?
	|_| no
	|_| yes

	Comment:      

	2.2 Top lift test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Test load / kg (≥ 6 mpgrw)
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Note: mpgrw = maximum permitted gross weight

	Hold time / min
	≥ 5
	     
	     
(only 1, 2, 3)
	|_|

	Loss of filling good
	no
	     
	     
(only 3)
	|_|

	Damages
	no
	     
	     
(only 1, 2, 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	2.3 Drop test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Test weight / kg (≥ 1 mpgrw)
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Note: mpgrw = maximum permitted gross weight

	Filling good
	     
	     
	     
(only 0, 1)
	|_|

	Angle of repose / °
	≤	     
	     
	     
(only 0, 1)
	|_|

	Bulk density / kg/m³
	≥	     
	     
	     
(only 0, 1)
	|_|

	Particel size / mm
	≤	     
	     
	     
(only 0, 1)
	|_|

	Drop height / m
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Drop orientation
	     
	     
	     
(only 1, 2, 3)
	|_|

	Loss of filling good
	no
	     
	     
(only 3)
	|_|

	|_| class 1 goods
	→ no crack
	     
	     
(only 0, 3)
	|_|

	Damages
	no
	     
	     
(only 1, 2, 3)
	|_|

	Hold time after lifting / min
	≥ 5
	     
	     
(only 1, 2, 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	2.4 Topple test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Test weight / kg (≥ 1 mpgrw)
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Note: mpgrw = maximum permitted gross weight

	Degree of filling / %
	≥ 95
	     
	     
(only 1, 2, 3)
	|_|

	Topple height / m
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Loss of filling good
	no
	     
	     
(only 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	2.5 Righting test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Test weight / kg (≥ 1 mpgrw)
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Note: mpgrw = maximum permitted gross weight

	Degree of filling / %
	≥ 95
	     
	     
(only 1, 2, 3)
	|_|

	Righting velocity / m/s
	≥ 0,1
	     
	     
(only 1, 2, 3)
	|_|

	Damages
	no
	     
	     
(only 1, 2, 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	3 Verification of design type conformity
by the surveillance assessor (for one design type)

	3.1 UN mark (and requirements as stated in the approval, if applicable)
	Result

	(alternatively, photographs can be submitted, marking height shall be stated)
	(see footer)
	OK

	Primary marks
	see below photo 
	     
(only 1, 2, 3)
	|_|

	   font height / mm
	     
	     
(only 1)
	|_|

	Comment:      

	Photo of UN mark

	
Note: Photos must be trimmed to the relevant area before insertion, as this is not possible in the model template. Depending on the design type, additional photos of the stacking load pictogram, date clock, bottom mark, etc. can be inserted.

	3.2 Verification of the specification of this design type
(e.g. design (according to the technical drawing incl. drawing number and incl. revision date/status), raw material name and properties, closure/s, dimensions incl. tolerances, tare mass)

	Characteristic checked
	Target
	Actual
	Result

	
	as per approval
	
	(see footer)
	OK

	Design
Drawing/sample comparison
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     	
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(0, 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	Additionally used documents:

	Approval certificate no. 
incl. revision date/status
	     

	if necessary:
Design type test report no.
	     

	Comment:      

	Which documentation is provided by the company to the user of this design type, e.g. packaging or closing instruction?

	Description:      
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[bookmark: _Hlk501695065]3 = safety-relevant non-conformity | recommendations can always be added in the comments field 	
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