	Surveillance protocol according to BAM-GGR 001
Metal large packagings
	



	Surveillance protocol no.
	     

	to surveillance visit report no.
	     



	1 Review of the company’s self-monitoring by the surveillance assessor
(tests and test frequencies according to BAM-GGR 001)

	The self-monitoring documentation was checked at random:

	Design type/s/
approval certificate no/s.:
	     

	Production period/s:
	     

	Tests
	Testing frequency
	Result

	
	Minimum
	Actual
	(see footer)
	OK

	Materials, i.e. sheets/coils
	1/delivery
	     
	     
	|_|

	only in case of external supplier:
Finished and semi-finished goods, e.g. closures
	1/delivery
	     
	     
	|_|

	Dimensions
(e.g. functional dimensions, wall thickness)
	1/(8 h) or
1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Visual checks
(e.g. joints, seams, inner condition)
	each
	     
	     
(only 1, 2, 3)
	|_|

	Gaskets/closures/valves
(correct assembly and function)
	1/(8 h) or
1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Mass of finished packaginga
	1/100 or
1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Marks
(correctness, readability, durability)
	1/(8 h) or
1/lot
	     
	     
(only 1, 2, 3)
	|_|

	only for large salvage packaging:
Leakproofness test
	1/lot
	     
	     
(0, 1, 2, 3)
	|_|

	Drop testb
	1/1500 or
1/(3 years)
	     
	     
(only 1, 2, 3)
	|_|

	if designed for it:
Stacking testb
	1/1500 or
1/(3 years) or exemptc
	     
	     
	|_|

	if designed for it:
Bottom lift testb
	1/1500 or
1/(3 years)
	     
	     
	|_|

	if designed for it:
Top lift testb
	1/1500 or
1/(3 years)
	     
	     
	|_|

	Notes:
a = calculation of overall mass by summing up the mass of the individual parts allowed
b = one sample can be used for all tests
c = only if a competent authority-issued written confirmation is available that this test need not to be done in course of the approval process

	Comment:      

	2 Tests (according to ADR)
by the company in presence of the surveillance assessor

	|_| Tests (according to ADR) are carried out completely or in part by an external body
(please complete 2.1a in this case)

	2.1 Testing facilities and measuring equipment for internal tests (according to ADR)

	Were there any changes to the testing facilities since last surveillance visit?
	|_| yes
	|_| no

	Comment:      

	Review of the …
	(see footer)
	OK

	testing facilities (availability and suitability)
	     
(only 1, 2, 3)
	|_|

	measuring equipment (availability and suitability [type and calibration range])
	     
(only 1, 2, 3)
	|_|

	Comment:      

	2.1a External testing (according to ADR), if applicable

	Which external body (name, place) is carrying out tests (according to ADR) on behalf of the company?

	     

	Is this external body named in the recognized QAP?
	|_| no
	|_| yes

	Comment:      

	2.2 Drop test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Gross mass / kg
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Filling good
	     
	     
	     
(only 0, 1)
	|_|

	Drop height / m
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Drop orientation
	     
	     
	     
(only 1, 2, 3)
	|_|

	Loss of filling good
	no
	     
	     
(only 3)
	|_|

	|_| class 1 goods
	→ no crack
	     
	     
(only 0, 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	the following test only if the large packaging is designed for it

	2.3 Stacking test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Stacking load / kg
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Hold time / min
	5
	     
	     
(only 1)
	|_|

	Loss of filling good
	no
	     
	     
(only 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	the following test only if the large packaging is designed for it

	2.4 Bottom lift test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Test mass / kg (≥ 1,25 mpgm)
	≥	     
	     
	     
(only 1, 2)
	|_|

	Note: mpgm = maximum permissible gross mass

	Number of raisings and lowerings
	2
	     
	     
(only 1)
	|_|

	Loss of filling good
	no
	     
	     
(only 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	the following test only if the large packaging is designed for it

	2.5 Top lift test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Test mass / kg (2 mpgm)
	≥	     
	     
	     
(only 1, 2)
	|_|

	Note: mpgm = maximum permissible gross mass

	Hold time / min
	5
	     
	     
(only 1)
	|_|

	Loss of filling good
	no
	     
	     
(only 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	only for large salvage packaging

	2.6 Leakproofness test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Test pressure / kPa
	≥ 30
	     
	     
(only 1, 2, 3)
	|_|

	Air leakage
	no
	     
	     
(only 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	3 Verification of design type conformity
by the surveillance assessor (for one design type)

	3.1 UN mark (and requirements as stated in the approval, if applicable)
	Result

	(alternatively, photographs can be submitted, marking height shall be stated)
	(see footer)
	OK

	UN mark
	see below photo 
	     
(only 1, 2, 3)
	|_|

	   font height / mm
	     
	     
(only 1)
	|_|

	Stacking load symbol
	|_| affixed
	|_| not affixed
	     
(only 1, 2)
	|_|

	   transport stacking
   load / kg
	     
	     
(only 0, 1, 2)
	|_|

	   font height / mm
	     
	     
(only 0, 1)
	|_|

	Comment:      

	Photo of UN mark

	
Note: Photos must be trimmed to the relevant area before insertion, as this is not possible in the model template. Depending on the design type, additional photos of the stacking load pictogram, date clock, bottom mark, etc. can be inserted.

	3.2 Verification of the specification of this design type
(e.g. design (according to the technical drawing incl. drawing number and incl. revision date/status), material thickness, closure/s, dimensions incl. tolerances, tare mass, fittings)

	Characteristic checked
	Target
	Actual
	Result

	
	as per approval
	
	(see footer)
	OK

	Design
Drawing/sample comparison
	     
	     
	     
(only 1, 2, 3)
	|_|

	Design closure
Drawing/sample comparison
	     	
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	Additionally used documents:

	Approval certificate no. 
incl. revision date/status
	     

	Design type test report no.
	     

	Comment:      

	Which documentation is provided by the company to the user of this design type, e.g. packaging or closing instruction?

	Description:      



	
[bookmark: _Hlk501705100]0 = not applicable, 1 = minor non-conformity 2 = serious non-conformity, 
[bookmark: _Hlk501695065]3 = safety-relevant non-conformity | recommendations can always be added in the comments field
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