	Surveillance protocol according to BAM-GGR 001
Remanufactured composite IBCs
	



	Surveillance protocol no.
	     

	to surveillance visit report no.
	     



	1 Review of the company’s self-monitoring by the surveillance assessor
(tests and test frequencies according to BAM-GGR 001)

	The self-monitoring documentation was checked at random:

	Design type/s/
approval certificate no/s.:
	     

	Production period/s:
	     

	Tests
	Testing frequency
	Result

	
	Minimum
	Actual
	(see footer)
	OK

	only in case of external supplier:
Inner receptacle
	1/delivery
	     
	     
	|_|

	Notes:	In this case the following parameters of the inner receptacle shall be checked by the remanufacturer based on the approval documents or proof shall be provided based on a certificate of the producer of the inner receptacle for the delivered batch: design incl. closures and fittings/valves, dimensions, mass, minimum wall thickness, marks incl. material code if stated in the approval certificate. A certificate of the producer of the inner receptacle with this information will be accepted if it contains a comparison of target and actual (delivered batch) values and if reference to the technical drawings of the relevant remanufacturing approval is given.
The production of the inner receptacle is reviewed in course of the surveillance of the manufacturing (new IBC), if the inner receptacle is not a supplied part, but is produced at the same site (result above: 0).

	only in case of external supplier:
Finished and semi-finished goods, e.g. closures
	1/delivery
	     
	     
	|_|

	Dimensions
(e.g. functional dimensions, wall thickness)
	1/(8 h) or
1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Correct assembly a,b
	1/(8 h) or
1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Visual checksa,b
(e.g. joints, seams, inner condition)
	1/(8 h) or
1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Marks on the inner receptacle
(correctness, readability, durability)b
	1/(8 h) or
1/lot
	     
	     
(only 1, 2, 3)
	|_|

	Original UN marks
removed or made permanently illegible
	each
	     
	     
(only 1, 2, 3)
	|_|

	Marks
(correctness, readability, durability)b
	each
	     
	     
(only 1, 2, 3)
	|_|

	only for code 21 or 31:
In-production leakproofness testb
	each
	     
	     
	|_|

	only for code 21 or 31:
Leakproofness test according to ADRb,c
	1/month or
exemptd
	     
	     
	|_|

	only for liquid fillings:
Hydraulic pressure testf
	1/7500e or
1/year
	     
	     
	|_|

	Proper function of the service equipmentb,g
	each
	     
	     
	|_|

	For notes see next page.

	Notes:
a = inspection of the outer casing for non-conformities, especially such non-conformities, which can damage the inner receptacle, and of the fastening elements (welding seams, joints etc.)
b = also part of the inspection and testing procedure before the IBC is put into service or after remanufacturing
c = reduction of test pressure to 10 kPa (0.1 bar) possible, if bubble test in a water bath with added soap solution is carried out or if leak detection spray is used at all openings and seams
d = only possible, if each IBC is tested for 10 min (ADR requirement)
e = small series regulation: 1 Test at/after overall production (all design types) of 7500 IBCs
f = tests, carried out in course of an additional design type test for a revision of the approval, can be included
g = confirmation based on a separately documented testing within a corporate group or on a delivery certificate is sufficient

	Comment:      

	2 Tests (according to ADR)
by the company in presence of the surveillance assessor

	|_| Tests (according to ADR) are carried out completely or in part by an external body
(please complete 2.1a in this case)

	2.1 Testing facilities and measuring equipment for internal tests (according to ADR)

	Were there any changes to the testing facilities since last surveillance visit?
	|_| yes
	|_| no

	Comment:      

	Review of the …
	(see footer)
	OK

	testing facilities (availability and suitability)
	     
(only 1, 2, 3)
	|_|

	measuring equipment (availability and suitability [type and calibration range])
	     
(only 1, 2, 3)
	|_|

	Comment:      

	2.1a External testing (according to ADR), if applicable

	Which external body (name, place) is carrying out tests (according to ADR) on behalf of the company?

	     

	Is this external body named in the recognized QAP?
	|_| no
	|_| yes

	Comment:      

	Next test only for IBC with code 21 or 31

	2.2 Leakproofness test according to ADR (monthly, 10-minute test)

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Test pressure (range) / kPa
	≥ 20
	     
	     
(only 1, 2, 3)
	|_|

	Hold time / min
	≥ 10
	     
	     
(only 1, 2, 3)
	|_|

	Air leakage
	no
	     
	     
(only 3)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	Next test only for liquid fillings

	2.3 Hydraulic pressure test

	Testing internally in course of the surveillance visit
	|_|

	Testing externally (see 2.1a), test report no.:      
	|_|

	internal test: Was the testing instruction revised since last surveillance visit?
	|_| yes
	|_| no

	internal test: Does the company follow this instruction in course of this visit?
	|_| no
	|_| yes

	
	Target
	Actual
	Result

	
	
	
	(see footer)
	OK

	Test pressure (range) / kPa
	≥	     
	     
	     
(only 1, 2, 3)
	|_|

	Degree of filling / %
	≥ 98
	     
	     
(only 1)
	|_|

	Hold time / min
	≥ 10
	     
	     
(only 1, 2, 3)
	|_|

	Loss of filling good
	no
	     
	     
(only 3)
	|_|

	Water temperature / °C
inside the IBC
	≥ 12
	     
	     
(only 1)
	|_|

	UN mark/s or design type/s/
approval certificate no/s.
	     

	Number and source of samples

	   pieces from running production/quality control,
   pieces of retained samples,    pieces from stock

	Comment:      

	3 Verification of design type conformity
by the surveillance assessor (for one design type)

	3.1 UN mark (and requirements as stated in the approval, if applicable)
	Result

	(alternatively, photographs can be submitted, marking height shall be stated)
	(see footer)
	OK

	Primary marks
	see below photo 
	     
(only 1, 2, 3)
	|_|

	   font height / mm
	     
	     
(only 1)
	|_|

	   mark to indicate the
   the remanufacturing
   as per approval
	     
	     
(only 0, 1)
	|_|

	Additional marks

	   Capacity / l
	     
	     
(only 1, 2)
	|_|

	   Tare mass / kg
	     
	     
(only 1, 2)
	|_|

	   Test pressure / kPa
	     
	     
(only 1, 2)
	|_|

	   Date of last
   leakproofness test
	     
	     
(only 0, 1)
	|_|

	   Date of last
   inspection
	     
	     
(only 0, 1)
	|_|

	Note:Inspection and (leakproofness) testing is subject to national legal regulations. For instance, there might be a national legal regulation that only notified bodies or accredited inspection bodies will receive a permission from the national competent authority to carry out inspection and testing of UN approved IBC or the national competent authority itself will carry out the inspection and testing.

	Stacking load symbol
	|_| affixed
	|_| not affixed
	     
(only 1, 2)
	|_|

	   transport stacking
   load / kg
	     
	     
(only 0, 1, 2)
	|_|

	   font height / mm
	     
	     
(only 0, 1)
	|_|

	mark on the
inner receptacle
	     
	     
(only 1, 2, 3)
	|_|

	   date clock/information
	     
	     
(only 1, 2)
	|_|

	   material code
   as per approval
	     
	     
(only 0, 1, 2)
	|_|

	Are the inner receptacle marks readily accessible when presented for carriage?
	|_| yes
	|_| no
	no rating

	If „no“, is a duplicate placed on the outer casing? it shall be preceded by the wording „Inner receptacle“
	|_| affixed
	|_| not affixed
	     
(only 1)
	|_|

	duplicate of the inner receptacle marks
	     
	     
(only 1, 2, 3)
	|_|

	Comment:      

	Photo of UN mark

	
Note: Photos must be trimmed to the relevant area before insertion, as this is not possible in the model template. Depending on the design type, additional photos of the stacking load pictogram, date clock, bottom mark, etc. can be inserted.

	3.2 Verification of the specification of this design type
(e.g. design (according to the technical drawing incl. drawing number and incl. revision date/status), raw material name and properties, wall thickness, closure/s, dimensions incl. tolerances, tare mass, fittings)

	Characteristic checked
	Target
	Actual
	Result

	
	as per approval
	
	(see footer)
	OK

	Design
Drawing/sample comparison
	     
	     
	     
(only 1, 2, 3)
	|_|

	Design closure/s
Drawing/sample comparison
	     	
	     
	     
(only 1, 2, 3)
	|_|

	Design bottom valve
Drawing/sample comparison
	     
	     
	     
(0, 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	     
	     
	     
	     
(only 1, 2, 3)
	|_|

	Additionally used documents:

	Approval certificate no. 
incl. revision date/status
	     

	if necessary:
Design type test report no.
	     

	Comment:      

	Which documentation is provided by the company to the user of this design type, e.g. packaging or closing instruction?

	Description:      



	
[bookmark: _Hlk501705100][bookmark: _Hlk185497376]0 = not applicable, 1 = minor non-conformity, 2 = serious non-conformity, 
[bookmark: _Hlk501695065]3 = safety-relevant non-conformity | recommendations can always be added in the comments field	
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