This entry applies only to aqueous solutions comprised of water, tetramethylammonium hydroxide (TMAH), and no more than 1 % of other constituents. Other formulations containing tetramethylammonium hydroxide shall be assigned to an appropriate generic or N.O.S. entry (e.g., UN No. 2927, TOXIC LIQUID, CORROSIVE, ORGANIC, N.O.S.), except as follows:

(a) Other formulations containing a surfactant in a concentration > 1 % and with not less than 8.75 % tetramethylammonium hydroxide shall be assigned to UN No. 2927, TOXIC LIQUID, CORROSIVE, ORGANIC, N.O.S., PG I; and 

(b) Other formulations containing a surfactant in a concentration > 1 % and with more than 2.38 % but less than 8.75 % tetramethylammonium hydroxide shall be assigned to UN No. 2927, TOXIC LIQUID, CORROSIVE, ORGANIC, N.O.S., PG II.