UN No. 1057 LIGHTERS complying with standard EN ISO 9994:2019 "Lighters - Safety Specification" and UN No. 1057 LIGHTER REFILLS, may be carried subject only to the provisions of 3.4.1 (a) to (f), 3.4.2 (except for the total gross mass of 30 kg), 3.4.3 (except for the total gross mass of 20 kg), 3.4.11 and 3.4.12, provided the following conditions are met:

(a)	The total gross mass of each package is not more than 10 kg;

(b)	Not more than 100 kg gross mass of such packages is carried in a wagon or vehicle or large container; and

(c)	Each outer packaging is clearly and durably marked with "UN 1057 LIGHTERS" or "UN 1057 LIGHTER REFILLS", as appropriate.
