The general provisions of 4.1.1 and 4.1.3 shall be met.

Inner packagings made of plastics, paper or fibre shall be sift-proof.
Large outer packagings made of flexible plastics (51H) shall be used with flexible inner packagings only.

Maximum capacity: 3 m³

Special packing provision L3:
NOTE: For UN Nos. 2208 and 3486, carriage by sea in large packagings is prohibited.