Part 4, Chapter 1 requirements must be met, including:

1) Compatibility requirements

- Substances must be compatible with their packagings as required by 4;1.1.3.

2) Closure requirements

- Closures must meet the requirements of 4;1.1.4.

For UN 3077 are intermediate bulk containers (IBCs) with a maximum net quantity not exceeding 1 000 kg are permitted. Each IBC must be in accorance with Chapter 6.5 of the United Nations Model Regulations and must bear the required UN mark.