Miscellaneous dangerous goods - lithium batteries or sodium ion batteries, Class 9
Symbol (seven vertical stripes in upper half); battery group, one brocken and emitting flame in lower half: black
Background: white
Figure "9" underlined in bottom corner

For transport of lithium batteries or sodium ion batteries in accordance to packing instruction 965 or 968 section IA or 966, 967, 969, 970, 976, 977 or 978 section I only the Lithium batteries or sodium ion batteries Class 9 label is necessary.
For transport of lithium batteries in accordance to packing instruction 965 or 968 section IB the Lithium batteries or sodium ion batteries Class 9 label and the Battery Mark are necessary.
For transport of lithium batteries or sodium ion batteries in accordance to packing instruction 966, 967, 969, 970, 977 or 978 section II only the Battery Mark is necessary.