This substance may be transported under provisions of Class 3 or Division 4.1 only if it is so packed that the percentage of diluent will not fall below that stated at any time during transport (see 2;3.1.4 and 2;4.2.4). In cases where the diluent is not stated, the substance must be packed so that the amount of explosive substance does not exceed the stated value.