S_KLASSE	S_VPGRUPPE	S_TEXT	S_SPRACHE
3	I	Siedebeginn <= 35 °C	D
3	I	Initial boiling point <= 35 °C	E
3	II	Flammpunkt < 23 °C, Siedebeginn > 35 °C	D
3	II	Flash-point < 23 °C, initial boiling point > 35 °C	E
3	III	23 °C <= Flammpunkt <= 60 °C	D
3	III	23 °C <= flash-point <= 60 °C	E
4.1	I	Desensibilisierter explosiver fester Stoff	D
4.1	I	Solid desensitized explosive	E
4.1	II	Entzündbarer fester Stoff	D
4.1	II	Flammable solid	E
4.1	III	Weniger gefährlich entzündbarer fester Stoff oder polymerisierender Stoff	D
4.1	III	Less dangerous flammable solid or polymerizing substance	E
4.2	I	Selbstentzündlicher (pyrophorer) Stoff	D
4.2	I	Substance liable to spontaneous combustion (pyrophoric)	E
4.2	II	Selbsterhitzungsfähiger Stoff	D
4.2	II	Self-heating substance	E
4.2	III	Weniger selbsterhitzungsfähiger Stoff	D
4.2	III	Slightly self-heating substance or article	E
4.3	I	Heftig mit Wasser reagierender Stoff	D
4.3	I	Substance which reacts vigorously with water	E
4.3	II	Leicht mit Wasser reagierender Stoff	D
4.3	II	Substance which reacts readily with water	E
4.3	III	Langsam mit Wasser reagierender Stoff	D
4.3	III	Substance which reacts slowly with water	E
5.1	I	Stark oxidierender Stoff	D
5.1	I	Highly oxidizing substance	E
5.1	II	Oxidierender Stoff	D
5.1	II	Oxidizing substance	E
5.1	III	Schwach oxidierender Stoff	D
5.1	III	Slightly oxidizing substance	E
6.1	I	Sehr giftiger Stoff	D
6.1	I	Highly toxic substance	E
6.1	II	Giftiger Stoff	D
6.1	II	Toxic substance	E
6.1	III	Schwach giftiger Stoff	D
6.1	III	Slightly toxic substance	E
8	I	Stark ätzender Stoff	D
8	I	Highly corrosive substance	E
8	II	Ätzender Stoff	D
8	II	Corrosive substance	E
8	III	Schwach ätzender Stoff	D
8	III	Slightly corrosive substance	E
9	II	Stoff mittlerer Gefahr	D
9	II	Substance presenting medium danger	E
9	III	Stoff geringer Gefahr	D
9	III	Substance presenting low danger	E
