For substances that must be stabilized for carriage and for which the SAPT is not more than that prescribed in 2.4.2.5.2, according to 3.1.2.6, the special provision 386 in Chapter 3.3 and the provisions in 7.3.7 shall also apply.

Special provisions 386 have been assigned to this substance for the DANGEROUS GOODS database in addition to the provisions in the Dangerous Goods List of the IMDG Code. Furthermore, according to 7.1.4.7, stuwage categorie 'D' and stowage code 'SW1' applies in deviation from the entry in column 16a of the Dangerous Goods List.

If, when transported in packagings or tanks, the substance has a self-accelerating polymerization temperature (SAPT) of more than 75°C and a heat of reaction not exceeding 300 J/g, these special provision need not be taken into account. BAM does not have any concrete values for this. It was therefore decided to list the special provision here.