This substance of packing group I shall not be transported or handed over for carriage in portable tanks in the molten state according to sub-section 4.2.1.19 of the RID because the assigned tank instruction in Table A, column 10 does not refer to carriage of the substance above its melting point. 

Because no tank code for liquids (L) is given for this substance according to Table A, column 12, carriage in RID tanks is also not possible. 

For this substance, carriage in the molten state is therefore prohibited.