The general provisions of 4.1.1, 4.1.2 and 4.1.3 and special provisions of 4.1.5 shall be met.

Additional requirements
1. IBCs shall only be used for free flowing substances.
2. Flexible IBCs shall only be used for solids.

Special packing provision B 10:
For UN No. 0241, this packing instruction may only be used for substances which consist of water as an essential ingredient and high proportions of ammonium nitrate or other oxidizing substances some or all of which are in solution. The other constituents may include hydrocarbons or aluminium powder, but shall not include nitro-derivatives such as trinitrotoluene. Metal IBCs are not authorized.