Special packing provisions PP 17 and PP 96:

PP 17: For UN No. 2037, packages shall not exceed 55 kg net mass for fibreboard packagings or 125 kg net mass for other packagings.

PP 96: For UN No. 2037 waste gas cartridges carried in accordance with special provision 327 of Chapter 3.3, the packagings shall be adequately ventilated to prevent the creation of dangerous atmospheres and the build-up of pressure.


Special packing provision RR 6 specific to RID:
For UN No. 2037, in the case of carriage by full load, metal articles may also be packed as follows:
The articles shall be grouped together in units on trays and held in position with an appropriate plastics cover; these units shall be stacked and suitably secured on pallets.